##############################################################
#
# Xilinx Core Generator version 14.2
# Date: Wed Aug 14 15:15:42 2013
#
##############################################################
#
#  This file contains the customisation parameters for a
#  Xilinx CORE Generator IP GUI. It is strongly recommended
#  that you do not manually alter this file as it may cause
#  unexpected and unsupported behavior.
#
##############################################################
#
#  Generated from component: xilinx.com:ip:fifo_generator:6.2
#
##############################################################
#
# BEGIN Project Options
SET addpads = false
SET asysymbol = true
SET busformat = BusFormatAngleBracketNotRipped
SET createndf = false
SET designentry = Verilog
SET device = xc4vfx20
SET devicefamily = virtex4
SET flowvendor = Other
SET formalverification = false
SET foundationsym = false
SET implementationfiletype = Ngc
SET package = ff672
SET removerpms = false
SET simulationfiles = Behavioral
SET speedgrade = -10
SET verilogsim = true
SET vhdlsim = false
# END Project Options
# BEGIN Select
SELECT Fifo_Generator family Xilinx,_Inc. 6.2
# END Select
# BEGIN Parameters
CSET almost_empty_flag=false
CSET almost_full_flag=false
CSET component_name=user_fifo
CSET data_count=false
CSET data_count_width=10
CSET disable_timing_violations=false
CSET dout_reset_value=0
CSET empty_threshold_assert_value=4
CSET empty_threshold_negate_value=5
CSET enable_ecc=false
CSET enable_int_clk=false
CSET enable_reset_synchronization=true
CSET fifo_implementation=Independent_Clocks_Distributed_RAM
CSET full_flags_reset_value=1
CSET full_threshold_assert_value=512
CSET full_threshold_negate_value=511
CSET inject_dbit_error=false
CSET inject_sbit_error=false
CSET input_data_width=32
CSET input_depth=1024
CSET output_data_width=32
CSET output_depth=1024
CSET overflow_flag=false
CSET overflow_sense=Active_High
CSET performance_options=First_Word_Fall_Through
CSET programmable_empty_type=No_Programmable_Empty_Threshold
CSET programmable_full_type=Multiple_Programmable_Full_Threshold_Constants
CSET read_clock_frequency=1
CSET read_data_count=false
CSET read_data_count_width=10
CSET reset_pin=true
CSET reset_type=Asynchronous_Reset
CSET underflow_flag=false
CSET underflow_sense=Active_High
CSET use_dout_reset=true
CSET use_embedded_registers=false
CSET use_extra_logic=false
CSET valid_flag=false
CSET valid_sense=Active_High
CSET write_acknowledge_flag=false
CSET write_acknowledge_sense=Active_High
CSET write_clock_frequency=1
CSET write_data_count=false
CSET write_data_count_width=10
# END Parameters
# BEGIN Extra information
MISC pkg_timestamp=2012-07-21T06:31:03Z
# END Extra information
GENERATE
# CRC: 75849c1f
