##############################################################
#
# Xilinx Core Generator version 14.2
# Date: Wed Aug 14 20:08:35 2013
#
##############################################################
#
#  This file contains the customisation parameters for a
#  Xilinx CORE Generator IP GUI. It is strongly recommended
#  that you do not manually alter this file as it may cause
#  unexpected and unsupported behavior.
#
##############################################################
#
#  Generated from component: xilinx.com:ip:fifo_generator:9.2
#
##############################################################
#
# BEGIN Project Options
SET addpads = false
SET asysymbol = true
SET busformat = BusFormatAngleBracketNotRipped
SET createndf = false
SET designentry = Verilog
SET device = xc4vfx20
SET devicefamily = virtex4
SET flowvendor = Other
SET formalverification = false
SET foundationsym = false
SET implementationfiletype = Ngc
SET package = ff672
SET removerpms = false
SET simulationfiles = Behavioral
SET speedgrade = -10
SET verilogsim = true
SET vhdlsim = false
# END Project Options
# BEGIN Select
SELECT Fifo_Generator xilinx.com:ip:fifo_generator:9.2
# END Select
# BEGIN Parameters
CSET add_ngc_constraint_axi=false
CSET almost_empty_flag=true
CSET almost_full_flag=false
CSET aruser_width=1
CSET awuser_width=1
CSET axi_address_width=32
CSET axi_data_width=64
CSET axi_type=AXI4_Stream
CSET axis_type=FIFO
CSET buser_width=1
CSET clock_enable_type=Slave_Interface_Clock_Enable
CSET clock_type_axi=Common_Clock
CSET component_name=read_fifo
CSET data_count=false
CSET data_count_width=10
CSET disable_timing_violations=false
CSET disable_timing_violations_axi=false
CSET dout_reset_value=0
CSET empty_threshold_assert_value=4
CSET empty_threshold_assert_value_axis=1022
CSET empty_threshold_assert_value_rach=1022
CSET empty_threshold_assert_value_rdch=1022
CSET empty_threshold_assert_value_wach=1022
CSET empty_threshold_assert_value_wdch=1022
CSET empty_threshold_assert_value_wrch=1022
CSET empty_threshold_negate_value=5
CSET enable_aruser=false
CSET enable_awuser=false
CSET enable_buser=false
CSET enable_common_overflow=false
CSET enable_common_underflow=false
CSET enable_data_counts_axis=false
CSET enable_data_counts_rach=false
CSET enable_data_counts_rdch=false
CSET enable_data_counts_wach=false
CSET enable_data_counts_wdch=false
CSET enable_data_counts_wrch=false
CSET enable_ecc=false
CSET enable_ecc_axis=false
CSET enable_ecc_rach=false
CSET enable_ecc_rdch=false
CSET enable_ecc_wach=false
CSET enable_ecc_wdch=false
CSET enable_ecc_wrch=false
CSET enable_read_channel=false
CSET enable_read_pointer_increment_by2=false
CSET enable_reset_synchronization=true
CSET enable_ruser=false
CSET enable_tdata=false
CSET enable_tdest=false
CSET enable_tid=false
CSET enable_tkeep=false
CSET enable_tlast=false
CSET enable_tready=true
CSET enable_tstrobe=false
CSET enable_tuser=false
CSET enable_write_channel=false
CSET enable_wuser=false
CSET fifo_application_type_axis=Data_FIFO
CSET fifo_application_type_rach=Data_FIFO
CSET fifo_application_type_rdch=Data_FIFO
CSET fifo_application_type_wach=Data_FIFO
CSET fifo_application_type_wdch=Data_FIFO
CSET fifo_application_type_wrch=Data_FIFO
CSET fifo_implementation=Common_Clock_Distributed_RAM
CSET fifo_implementation_axis=Common_Clock_Block_RAM
CSET fifo_implementation_rach=Common_Clock_Block_RAM
CSET fifo_implementation_rdch=Common_Clock_Block_RAM
CSET fifo_implementation_wach=Common_Clock_Block_RAM
CSET fifo_implementation_wdch=Common_Clock_Block_RAM
CSET fifo_implementation_wrch=Common_Clock_Block_RAM
CSET full_flags_reset_value=1
CSET full_threshold_assert_value=510
CSET full_threshold_assert_value_axis=1023
CSET full_threshold_assert_value_rach=1023
CSET full_threshold_assert_value_rdch=1023
CSET full_threshold_assert_value_wach=1023
CSET full_threshold_assert_value_wdch=1023
CSET full_threshold_assert_value_wrch=1023
CSET full_threshold_negate_value=509
CSET id_width=4
CSET inject_dbit_error=false
CSET inject_dbit_error_axis=false
CSET inject_dbit_error_rach=false
CSET inject_dbit_error_rdch=false
CSET inject_dbit_error_wach=false
CSET inject_dbit_error_wdch=false
CSET inject_dbit_error_wrch=false
CSET inject_sbit_error=false
CSET inject_sbit_error_axis=false
CSET inject_sbit_error_rach=false
CSET inject_sbit_error_rdch=false
CSET inject_sbit_error_wach=false
CSET inject_sbit_error_wdch=false
CSET inject_sbit_error_wrch=false
CSET input_data_width=32
CSET input_depth=512
CSET input_depth_axis=1024
CSET input_depth_rach=16
CSET input_depth_rdch=1024
CSET input_depth_wach=16
CSET input_depth_wdch=1024
CSET input_depth_wrch=16
CSET interface_type=Native
CSET output_data_width=32
CSET output_depth=512
CSET overflow_flag=false
CSET overflow_flag_axi=false
CSET overflow_sense=Active_High
CSET overflow_sense_axi=Active_High
CSET performance_options=First_Word_Fall_Through
CSET programmable_empty_type=No_Programmable_Empty_Threshold
CSET programmable_empty_type_axis=No_Programmable_Empty_Threshold
CSET programmable_empty_type_rach=No_Programmable_Empty_Threshold
CSET programmable_empty_type_rdch=No_Programmable_Empty_Threshold
CSET programmable_empty_type_wach=No_Programmable_Empty_Threshold
CSET programmable_empty_type_wdch=No_Programmable_Empty_Threshold
CSET programmable_empty_type_wrch=No_Programmable_Empty_Threshold
CSET programmable_full_type=Multiple_Programmable_Full_Threshold_Constants
CSET programmable_full_type_axis=No_Programmable_Full_Threshold
CSET programmable_full_type_rach=No_Programmable_Full_Threshold
CSET programmable_full_type_rdch=No_Programmable_Full_Threshold
CSET programmable_full_type_wach=No_Programmable_Full_Threshold
CSET programmable_full_type_wdch=No_Programmable_Full_Threshold
CSET programmable_full_type_wrch=No_Programmable_Full_Threshold
CSET rach_type=FIFO
CSET rdch_type=FIFO
CSET read_clock_frequency=1
CSET read_data_count=false
CSET read_data_count_width=10
CSET register_slice_mode_axis=Fully_Registered
CSET register_slice_mode_rach=Fully_Registered
CSET register_slice_mode_rdch=Fully_Registered
CSET register_slice_mode_wach=Fully_Registered
CSET register_slice_mode_wdch=Fully_Registered
CSET register_slice_mode_wrch=Fully_Registered
CSET reset_pin=true
CSET reset_type=Asynchronous_Reset
CSET ruser_width=1
CSET synchronization_stages=2
CSET synchronization_stages_axi=2
CSET tdata_width=64
CSET tdest_width=4
CSET tid_width=8
CSET tkeep_width=4
CSET tstrb_width=4
CSET tuser_width=4
CSET underflow_flag=false
CSET underflow_flag_axi=false
CSET underflow_sense=Active_High
CSET underflow_sense_axi=Active_High
CSET use_clock_enable=false
CSET use_dout_reset=true
CSET use_embedded_registers=false
CSET use_extra_logic=true
CSET valid_flag=false
CSET valid_sense=Active_High
CSET wach_type=FIFO
CSET wdch_type=FIFO
CSET wrch_type=FIFO
CSET write_acknowledge_flag=false
CSET write_acknowledge_sense=Active_High
CSET write_clock_frequency=1
CSET write_data_count=false
CSET write_data_count_width=10
CSET wuser_width=1
# END Parameters
# BEGIN Extra information
MISC pkg_timestamp=2012-06-23T13:35:37Z
# END Extra information
GENERATE
# CRC:  b3f7c29
