
################################################################################
##$Date: 2010/01/20 09:54:44 $
##$RCSfile: mgt_attributes_ucf.ejava,v $
##$Revision: 1.2 $
################################################################################
##   ____  ____ 
##  /   /\/   / 
## /___/  \  /    Vendor: Xilinx 
## \   \   \/     Version : 1.7
##  \   \         Application : RocketIO Wizard 
##  /   /         Filename : mgt_attributes.ucf
## /___/   /\     Timestamp : 02/08/2005 09:12:43
## \   \  /  \ 
##  \___\/\___\ 
##
##
## MGT ATTRIBUTES 
## This file contains the attributes for the active and unused MGTs in the
## design. If you would like to use this files in your design, please make
## sure that the path to the MGT instance is correct.
## Generated by Xilinx RocketIO Wizard
##

############################## Active MGT Attributes #######################

 ##-------- RocketIO MGT 64B66B Block Sync State Machine Attributes --------- 
 
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 SH_CNT_MAX              = 64;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 SH_INVALID_CNT_MAX      = 16;
 
 ##--------------------- RocketIO MGT Alignment Atrributes ------------------   
 
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 ALIGN_COMMA_WORD        = 4;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 COMMA_10B_MASK          = 10'h3ff;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 COMMA32                 = FALSE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 DEC_MCOMMA_DETECT       = TRUE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 DEC_PCOMMA_DETECT       = TRUE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 DEC_VALID_COMMA_ONLY    = TRUE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 MCOMMA_32B_VALUE        = 32'h0000017c;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 MCOMMA_DETECT           = TRUE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 PCOMMA_32B_VALUE        = 32'h00000283;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 PCOMMA_DETECT           = TRUE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 PCS_BIT_SLIP            = FALSE;    
  
 ##-- RocketIO MGT Atrributes Common to Clk Correction & Channel Bonding ----   
 
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 CCCB_ARBITRATOR_DISABLE = FALSE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 CLK_COR_8B10B_DE        = TRUE;    
 
 ##----------------- RocketIO MGT Channel Bonding Atrributes ----------------   
 
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 CHAN_BOND_LIMIT         = 16;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 CHAN_BOND_MODE          = NONE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 CHAN_BOND_ONE_SHOT      = FALSE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 CHAN_BOND_SEQ_1_1       = 11'b00000000000;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 CHAN_BOND_SEQ_1_2       = 11'b00000000000;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 CHAN_BOND_SEQ_1_3       = 11'b00000000000;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 CHAN_BOND_SEQ_1_4       = 11'b00000000000;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 CHAN_BOND_SEQ_1_MASK    = 4'b1110;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 CHAN_BOND_SEQ_2_1       = 11'b00000000000;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 CHAN_BOND_SEQ_2_2       = 11'b00000000000;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 CHAN_BOND_SEQ_2_3       = 11'b00000000000;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 CHAN_BOND_SEQ_2_4       = 11'b00000000000;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 CHAN_BOND_SEQ_2_MASK    = 4'b1111;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 CHAN_BOND_SEQ_2_USE     = FALSE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 CHAN_BOND_SEQ_LEN       = 1;    

 ##---------------- RocketIO MGT Clock Correction Atrributes ----------------   

 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 CLK_COR_MAX_LAT         = 40;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 CLK_COR_MIN_LAT         = 28;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 CLK_COR_SEQ_1_1         = 11'b00101111100;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 CLK_COR_SEQ_1_2         = 11'b00010010101;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 CLK_COR_SEQ_1_3         = 11'b00010110101;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 CLK_COR_SEQ_1_4         = 11'b00010110101;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 CLK_COR_SEQ_1_MASK      = 4'b0000;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 CLK_COR_SEQ_2_1         = 11'b00110111100;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 CLK_COR_SEQ_2_2         = 11'b00001001010;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 CLK_COR_SEQ_2_3         = 11'b00001001010;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 CLK_COR_SEQ_2_4         = 11'b00001111011;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 CLK_COR_SEQ_2_MASK      = 4'b0000;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 CLK_COR_SEQ_2_USE       = TRUE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 CLK_COR_SEQ_DROP        = FALSE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 CLK_COR_SEQ_LEN         = 4;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 CLK_CORRECT_USE         = FALSE;    
 
 ##-------------------- RocketIO MGT Clocking Atrributes --------------------      

 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 RX_CLOCK_DIVIDER        = 2'b11;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 RXASYNCDIVIDE           = 2'b10;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 RXCLK0_FORCE_PMACLK     = FALSE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 RXCLKMODE               = 6'b000011;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 RXOUTDIV2SEL            = 4;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 RXPLLNDIVSEL            = 20;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 RXPMACLKSEL             = REFCLK1;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 RXRECCLK1_USE_SYNC      = FALSE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 RXUSRDIVISOR            = 1;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 TX_CLOCK_DIVIDER        = 2'b11;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 TXABPMACLKSEL           = REFCLK1;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 TXASYNCDIVIDE           = 2'b10;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 TXCLK0_FORCE_PMACLK     = FALSE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 TXCLKMODE               = 4'b0100;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 TXOUTCLK1_USE_SYNC      = FALSE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 TXOUTDIV2SEL            = 4;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 TXPHASESEL              = TRUE; 
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 TXPLLNDIVSEL            = 20;

 ##------------------------ RocketIO MGT CRC Atrributes ---------------------   

 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 RXCRCCLOCKDOUBLE        = FALSE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 RXCRCENABLE             = FALSE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 RXCRCINITVAL            = 32'h00000000;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 RXCRCINVERTGEN          = FALSE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 RXCRCSAMECLOCK          = TRUE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 TXCRCCLOCKDOUBLE        = FALSE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 TXCRCENABLE             = FALSE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 TXCRCINITVAL            = 32'h00000000;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 TXCRCINVERTGEN          = FALSE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 TXCRCSAMECLOCK          = TRUE;
     
 ##------------------- RocketIO MGT Data Path Atrributes --------------------   

 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 RXDATA_SEL              = 2'b11;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 TXDATA_SEL              = 2'b10;

 ##-------------- RocketIO MGT Digital Receiver Attributes ------------------   

 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 DIGRX_FWDCLK            = 2'b00;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 DIGRX_SYNC_MODE         = TRUE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 ENABLE_DCDR             = FALSE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 RXBY_32                 = FALSE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 RXDIGRESET              = FALSE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 RXDIGRX                 = FALSE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 SAMPLE_8X               = FALSE;

 ##--------------- Rocket IO MGT Miscellaneous Attributes ------------------     

 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 GT11_MODE               = B;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 OPPOSITE_SELECT         = FALSE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 PMA_BIT_SLIP            = FALSE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 REPEATER                = FALSE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 RX_BUFFER_USE           = FALSE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 RXCDRLOS                = 6'b000110;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 RXDCCOUPLE              = FALSE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 RXFDCAL_CLOCK_DIVIDE    = NONE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 TX_BUFFER_USE           = FALSE;     
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 TXFDCAL_CLOCK_DIVIDE    = NONE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 TXSLEWRATE              = TRUE;

 ##--------------- Rocket IO MGT Preemphasis and Equalization --------------
 
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 RXAFEEQ                  = 9'b000000000;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 RXEQ                     = 64'h4000000000000000;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 TXDAT_PRDRV_DAC          = 3'b111;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 TXDAT_TAP_DAC            = 5'b10110;    
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 TXHIGHSIGNALEN           = TRUE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 TXPOST_PRDRV_DAC         = 3'b111;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 TXPOST_TAP_DAC           = 5'b00001;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 TXPOST_TAP_PD            = TRUE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 TXPRE_PRDRV_DAC          = 3'b111;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 TXPRE_TAP_DAC            = 5'b00000;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 TXPRE_TAP_PD             = TRUE;           
 

 ##--------------------- Restricted RocketIO MGT Attributes -------------------  

 ##/Note : THE FOLLOWING ATTRIBUTES ARE RESTRICTED. PLEASE DO NOT EDIT.

 ##--------------------------- Restricted: Biasing -------------------------
 
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 BANDGAPSEL               = FALSE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 BIASRESSEL               = FALSE;    
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 IREFBIASMODE             = 2'b11;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 PMAIREFTRIM              = 4'b0111;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 PMAVREFTRIM              = 4'b0111;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 TXAREFBIASSEL            = TRUE; 
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 TXTERMTRIM               = 4'b1100;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 VREFBIASMODE             = 2'b11;

 ##-------------- Restricted: Frequency Detector and Calibration -----------   
  
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 CYCLE_LIMIT_SEL          = 2'b00;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 FDET_HYS_CAL             = 3'b010;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 FDET_HYS_SEL             = 3'b100;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 FDET_LCK_CAL             = 3'b101;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 FDET_LCK_SEL             = 3'b001;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 LOOPCAL_WAIT             = 2'b00;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 RXCYCLE_LIMIT_SEL        = 2'b00;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 RXFDET_HYS_CAL           = 3'b010;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 RXFDET_HYS_SEL           = 3'b100;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 RXFDET_LCK_CAL           = 3'b101;   
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 RXFDET_LCK_SEL           = 3'b001;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 RXLOOPCAL_WAIT           = 2'b00;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 RXSLOWDOWN_CAL           = 2'b00;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 SLOWDOWN_CAL             = 2'b00;
 
 ##------------------------- Restricted: PLL Settings ----------------------
 
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 PMACLKENABLE             = TRUE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 PMACOREPWRENABLE         = TRUE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 PMAVBGCTRL               = 5'b00000;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 RXACTST                  = FALSE;       
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 RXAFETST                 = FALSE;      
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 RXCMADJ                  = 2'b01;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 RXCPSEL                  = FALSE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 RXCPTST                  = FALSE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 RXCTRL1                  = 10'h200;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 RXFECONTROL1             = 2'b00; 
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 RXFECONTROL2             = 3'b000; 
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 RXFETUNE                 = 2'b01; 
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 RXLKADJ                  = 5'b00000;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 RXLOOPFILT               = 4'b1111;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 RXPDDTST                 = TRUE;      
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 RXRCPADJ                 = 3'b011; 
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 RXRIBADJ                 = 2'b11;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 RXVCO_CTRL_ENABLE        = TRUE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 RXVCODAC_INIT            = 10'b0000101001;   
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 TXCPSEL                  = FALSE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 TXCTRL1                  = 10'h200;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 TXLOOPFILT               = 4'b1101;   
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 VCO_CTRL_ENABLE          = TRUE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 VCODAC_INIT              = 10'b0000101001;
 
 ##------------------------- Restricted: Powerdowns ------------------------
  
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 POWER_ENABLE             = TRUE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 RXAFEPD                  = FALSE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 RXAPD                    = FALSE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 RXLKAPD                  = FALSE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 RXPD                     = FALSE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 RXRCPPD                  = FALSE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 RXRPDPD                  = FALSE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 RXRSDPD                  = FALSE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 TXAPD                    = FALSE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 TXDIGPD                  = FALSE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 TXLVLSHFTPD              = FALSE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT0 TXPD                     = FALSE;
 ##-------- RocketIO MGT 64B66B Block Sync State Machine Attributes --------- 
 
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 SH_CNT_MAX              = 64;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 SH_INVALID_CNT_MAX      = 16;
 
 ##--------------------- RocketIO MGT Alignment Atrributes ------------------   
 
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 ALIGN_COMMA_WORD        = 4;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 COMMA_10B_MASK          = 10'h3ff;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 COMMA32                 = FALSE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 DEC_MCOMMA_DETECT       = TRUE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 DEC_PCOMMA_DETECT       = TRUE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 DEC_VALID_COMMA_ONLY    = TRUE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 MCOMMA_32B_VALUE        = 32'h0000017c;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 MCOMMA_DETECT           = TRUE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 PCOMMA_32B_VALUE        = 32'h00000283;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 PCOMMA_DETECT           = TRUE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 PCS_BIT_SLIP            = FALSE;    
  
 ##-- RocketIO MGT Atrributes Common to Clk Correction & Channel Bonding ----   
 
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 CCCB_ARBITRATOR_DISABLE = FALSE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 CLK_COR_8B10B_DE        = TRUE;    
 
 ##----------------- RocketIO MGT Channel Bonding Atrributes ----------------   
 
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 CHAN_BOND_LIMIT         = 16;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 CHAN_BOND_MODE          = NONE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 CHAN_BOND_ONE_SHOT      = FALSE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 CHAN_BOND_SEQ_1_1       = 11'b00000000000;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 CHAN_BOND_SEQ_1_2       = 11'b00000000000;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 CHAN_BOND_SEQ_1_3       = 11'b00000000000;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 CHAN_BOND_SEQ_1_4       = 11'b00000000000;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 CHAN_BOND_SEQ_1_MASK    = 4'b1110;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 CHAN_BOND_SEQ_2_1       = 11'b00000000000;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 CHAN_BOND_SEQ_2_2       = 11'b00000000000;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 CHAN_BOND_SEQ_2_3       = 11'b00000000000;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 CHAN_BOND_SEQ_2_4       = 11'b00000000000;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 CHAN_BOND_SEQ_2_MASK    = 4'b1111;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 CHAN_BOND_SEQ_2_USE     = FALSE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 CHAN_BOND_SEQ_LEN       = 1;    

 ##---------------- RocketIO MGT Clock Correction Atrributes ----------------   

 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 CLK_COR_MAX_LAT         = 40;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 CLK_COR_MIN_LAT         = 28;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 CLK_COR_SEQ_1_1         = 11'b00101111100;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 CLK_COR_SEQ_1_2         = 11'b00010010101;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 CLK_COR_SEQ_1_3         = 11'b00010110101;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 CLK_COR_SEQ_1_4         = 11'b00010110101;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 CLK_COR_SEQ_1_MASK      = 4'b0000;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 CLK_COR_SEQ_2_1         = 11'b00110111100;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 CLK_COR_SEQ_2_2         = 11'b00001001010;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 CLK_COR_SEQ_2_3         = 11'b00001001010;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 CLK_COR_SEQ_2_4         = 11'b00001111011;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 CLK_COR_SEQ_2_MASK      = 4'b0000;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 CLK_COR_SEQ_2_USE       = TRUE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 CLK_COR_SEQ_DROP        = FALSE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 CLK_COR_SEQ_LEN         = 4;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 CLK_CORRECT_USE         = FALSE;    
 
 ##-------------------- RocketIO MGT Clocking Atrributes --------------------      

 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 RX_CLOCK_DIVIDER        = 2'b11;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 RXASYNCDIVIDE           = 2'b10;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 RXCLK0_FORCE_PMACLK     = FALSE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 RXCLKMODE               = 6'b000011;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 RXOUTDIV2SEL            = 4;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 RXPLLNDIVSEL            = 20;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 RXPMACLKSEL             = REFCLK1;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 RXRECCLK1_USE_SYNC      = FALSE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 RXUSRDIVISOR            = 1;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 TX_CLOCK_DIVIDER        = 2'b11;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 TXABPMACLKSEL           = REFCLK1;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 TXASYNCDIVIDE           = 2'b10;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 TXCLK0_FORCE_PMACLK     = FALSE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 TXCLKMODE               = 4'b0100;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 TXOUTCLK1_USE_SYNC      = FALSE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 TXOUTDIV2SEL            = 4;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 TXPHASESEL              = TRUE; 
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 TXPLLNDIVSEL            = 20;

 ##------------------------ RocketIO MGT CRC Atrributes ---------------------   

 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 RXCRCCLOCKDOUBLE        = FALSE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 RXCRCENABLE             = FALSE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 RXCRCINITVAL            = 32'h00000000;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 RXCRCINVERTGEN          = FALSE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 RXCRCSAMECLOCK          = TRUE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 TXCRCCLOCKDOUBLE        = FALSE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 TXCRCENABLE             = FALSE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 TXCRCINITVAL            = 32'h00000000;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 TXCRCINVERTGEN          = FALSE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 TXCRCSAMECLOCK          = TRUE;
     
 ##------------------- RocketIO MGT Data Path Atrributes --------------------   

 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 RXDATA_SEL              = 2'b11;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 TXDATA_SEL              = 2'b10;

 ##-------------- RocketIO MGT Digital Receiver Attributes ------------------   

 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 DIGRX_FWDCLK            = 2'b00;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 DIGRX_SYNC_MODE         = TRUE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 ENABLE_DCDR             = FALSE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 RXBY_32                 = FALSE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 RXDIGRESET              = FALSE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 RXDIGRX                 = FALSE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 SAMPLE_8X               = FALSE;

 ##--------------- Rocket IO MGT Miscellaneous Attributes ------------------     

 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 GT11_MODE               = A;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 OPPOSITE_SELECT         = FALSE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 PMA_BIT_SLIP            = FALSE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 REPEATER                = FALSE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 RX_BUFFER_USE           = FALSE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 RXCDRLOS                = 6'b000110;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 RXDCCOUPLE              = FALSE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 RXFDCAL_CLOCK_DIVIDE    = NONE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 TX_BUFFER_USE           = FALSE;     
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 TXFDCAL_CLOCK_DIVIDE    = NONE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 TXSLEWRATE              = TRUE;

 ##--------------- Rocket IO MGT Preemphasis and Equalization --------------
 
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 RXAFEEQ                  = 9'b000000000;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 RXEQ                     = 64'h4000000000000000;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 TXDAT_PRDRV_DAC          = 3'b111;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 TXDAT_TAP_DAC            = 5'b10110;    
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 TXHIGHSIGNALEN           = TRUE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 TXPOST_PRDRV_DAC         = 3'b111;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 TXPOST_TAP_DAC           = 5'b00001;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 TXPOST_TAP_PD            = TRUE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 TXPRE_PRDRV_DAC          = 3'b111;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 TXPRE_TAP_DAC            = 5'b00000;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 TXPRE_TAP_PD             = TRUE;           
 

 ##--------------------- Restricted RocketIO MGT Attributes -------------------  

 ##/Note : THE FOLLOWING ATTRIBUTES ARE RESTRICTED. PLEASE DO NOT EDIT.

 ##--------------------------- Restricted: Biasing -------------------------
 
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 BANDGAPSEL               = FALSE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 BIASRESSEL               = FALSE;    
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 IREFBIASMODE             = 2'b11;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 PMAIREFTRIM              = 4'b0111;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 PMAVREFTRIM              = 4'b0111;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 TXAREFBIASSEL            = TRUE; 
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 TXTERMTRIM               = 4'b1100;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 VREFBIASMODE             = 2'b11;

 ##-------------- Restricted: Frequency Detector and Calibration -----------   
  
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 CYCLE_LIMIT_SEL          = 2'b00;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 FDET_HYS_CAL             = 3'b010;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 FDET_HYS_SEL             = 3'b100;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 FDET_LCK_CAL             = 3'b101;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 FDET_LCK_SEL             = 3'b001;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 LOOPCAL_WAIT             = 2'b00;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 RXCYCLE_LIMIT_SEL        = 2'b00;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 RXFDET_HYS_CAL           = 3'b010;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 RXFDET_HYS_SEL           = 3'b100;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 RXFDET_LCK_CAL           = 3'b101;   
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 RXFDET_LCK_SEL           = 3'b001;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 RXLOOPCAL_WAIT           = 2'b00;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 RXSLOWDOWN_CAL           = 2'b00;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 SLOWDOWN_CAL             = 2'b00;
 
 ##------------------------- Restricted: PLL Settings ----------------------
 
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 PMACLKENABLE             = TRUE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 PMACOREPWRENABLE         = TRUE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 PMAVBGCTRL               = 5'b00000;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 RXACTST                  = FALSE;       
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 RXAFETST                 = FALSE;      
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 RXCMADJ                  = 2'b01;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 RXCPSEL                  = FALSE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 RXCPTST                  = FALSE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 RXCTRL1                  = 10'h200;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 RXFECONTROL1             = 2'b00; 
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 RXFECONTROL2             = 3'b000; 
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 RXFETUNE                 = 2'b01; 
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 RXLKADJ                  = 5'b00000;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 RXLOOPFILT               = 4'b1111;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 RXPDDTST                 = TRUE;      
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 RXRCPADJ                 = 3'b011; 
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 RXRIBADJ                 = 2'b11;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 RXVCO_CTRL_ENABLE        = TRUE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 RXVCODAC_INIT            = 10'b0000101001;   
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 TXCPSEL                  = FALSE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 TXCTRL1                  = 10'h200;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 TXLOOPFILT               = 4'b1101;   
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 VCO_CTRL_ENABLE          = TRUE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 VCODAC_INIT              = 10'b0000101001;
 
 ##------------------------- Restricted: Powerdowns ------------------------
  
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 POWER_ENABLE             = TRUE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 RXAFEPD                  = FALSE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 RXAPD                    = FALSE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 RXLKAPD                  = FALSE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 RXPD                     = FALSE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 RXRCPPD                  = FALSE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 RXRPDPD                  = FALSE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 RXRSDPD                  = FALSE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 TXAPD                    = FALSE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 TXDIGPD                  = FALSE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 TXLVLSHFTPD              = FALSE;
 INST sata_core_i/sata_phy_i/rocketio_i/MGT1 TXPD                     = FALSE;




